{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,0,0,10]],"flags":["formulas_cached_only"]}
["FY 12 Army Ground Reimbursable Rates"]
["LIN","MDS Name","REPARABLE per Mile","CONSUMABLE per Mile","POL          per Mile","Total Reparable, Consumable & POL Per Day","LOGSA Veh Cost","Vehicle Depreciated Usage Factor per Day ","DoD Crew per DAY Rate (2pax)","Army Reimbursable Rate per Day w/out Crew Pay","Army Reimbursable Rate per Day w/ Crew Pay"]
["T59048","HET Series                         ",1.881882242254927,3.2878373318740817,1.06,56.27509522725815,256704,56.346528,611.5164615384615,112.62162322725814,724.1380847657197]
["T61103","M915/6 Series                       ",0.12,0.53,0.53,36.65469283131074,162968,35.771476,611.5164615384615,72.42616883131075,683.9426303697722]
["T07679","HVY HMMWV  Series                     ",0.19,0.99,0.21,18.89821613789202,102148,22.421485999999998,611.5164615384615,41.31970213789202,652.8361636763535]
["T38844","HMMWV AMB Series",0.34,1.5899999999999999,0.21,27.952538907753258,113998,25.022560999999996,611.5164615384615,52.975099907753254,664.4915614462147]
["T41036","MTV Series",0.17,1.8199999999999998,0.56,20.05929493999703,118579,26.028090499999998,611.5164615384615,46.08738543999703,657.6038469784585]
["T41995","LMTV SERIES                       ",0.27,1.58,0.47,20.298510742085217,103220,22.656789999999997,611.5164615384615,42.955300742085214,654.4717622805467]
["T92446","UP-ARMORED SERIES                         ",0.19,1.13,0.21,29.85726183686307,146844,32.232257999999995,611.5164615384615,62.08951983686306,673.6059813753245]
["T91656","M917 SERIES               ",0.87,4.66,0.53,26.47367185086003,166223,36.4859485,611.5164615384615,62.95962035086003,674.4760818893216]
["T43784","M939 SERIES                    ",0.8016498137307078,2.404555614688664,0.56,24.525862689734304,98341,21.5858495,611.5164615384615,46.111712189734305,657.6281737281959]
["T96496","HEMTT SERIES                       ",1.42,2.86,1.24,49.962084210526314,226800,49.782599999999995,611.5164615384615,99.74468421052632,711.2611457489878]
["X40009","M35 SERIES",0.11,1.69,0.38,22.290472039623523,176428,38.72594599999999,611.5164615384615,61.01641803962352,672.532879578085]
["T05028","CUCV SERIES                       ",0.01,0.55,0.24,5.417246885329266,32990,7.241305,611.5164615384615,12.658551885329267,624.1750134237908]
["T61494","HMMWV SERIES                         ",0.3,1.42,0.21,24.016937404118977,102148,22.421485999999998,611.5164615384615,46.43842340411898,657.9548849425805]
["T40999","PLS SERIES                         ",0.8,3.2800000000000002,1.24,48.49812652939421,360139,79.0505105,611.5164615384615,127.54863702939421,739.0650985678557]
["T87243","HEMTT Fueler",1.42,2.86,1.24,49.962084210526314,268440,58.922579999999996,611.5164615384615,108.88466421052631,720.4011257489879]
["X43708","M809 SERIES                          ",0.8016498137307078,2.404555614688664,0.56,24.525862689734304,176428,38.72594599999999,611.5164615384615,63.2518086897343,674.7682702281958]
["T96883","Small Trailers",null,null,null,6.375548003903217,14423,3.1658484999999996,374.9178305860806,9.541396503903217,384.4592270899838]
["T93761","Large Trailers",null,null,null,6.375548003903217,46731,10.2574545,562.983409035409,16.633002503903217,579.6164115393121]
["G36169","2KW",null,null,null,0.3290605421369402,6000,1.317,374.9178305860806,1.64606054213694,376.5638911282175]
["G74847","3KW",null,null,null,0.5038739551471897,9348,2.0518859999999997,374.9178305860806,2.5557599551471895,377.4735905412278]
["G42238","5KW",null,null,null,1.614453284859363,23738,5.210491,374.9178305860806,6.824944284859363,381.74277487093997]
["G38140","10KW",null,null,null,2.1080440980647728,26333,5.7800935,374.9178305860806,7.888137598064773,382.80596818414534]
["J35595","60KW",null,null,null,5.285534958074602,33805,7.4201975,374.9178305860806,12.705732458074602,387.62356304415516]
["W37243","RAWS/TWPS",null,null,null,6.673759120214819,320518,70.353701,562.983409035409,77.02746012021483,640.0108691556238]
["W35417","ROWPU",null,null,null,34.78786918903965,86600,19.008699999999997,374.9178305860806,53.796569189039644,428.7143997751202]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}