{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["FY 10 Final"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"FY 10 Final","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[[0,1,0,11],[11,1,11,13]],"flags":["formulas_cached_only"]}
[null,"FY10 DOD Fixed Wing Aviation Reimbursable Rates"]
[null,"Aircraft","FY","Fuel","Other CLS per MH","Other Per Diem Pay","Crew Pay","Asset Utilization","DoD Rate","Other FED AGY","FMS","Public Rate"]
[null,"RC 12","10",307,1340,28.882,171.60469293,67.03528,1647,1675.882,1847.4866929300001,1914.5219729300002]
[null,"C-12","10",307,1041,28.882,171.60469293,55.07528000000001,1348,1376.882,1548.4866929300001,1603.5619729300001]
[null,"C-20","10",1952.5,3663,221.7725,286.32461582999997,233.4909,5615.5,5837.2725,6123.59711583,6357.08801583]
[null,"C-23","10",303,1890,23.724500000000003,228.96465438,88.66897999999999,2193,2216.7245,2445.6891543799998,2534.3581343799997]
[null,"C-26","10",210,1189,24.756,228.96465438,56.95024000000001,1399,1423.756,1652.72065438,1709.67089438]
[null,"C-37","10",215,5290,221.7725,286.32461582999997,229.0709,5505,5726.7725,6013.09711583,6242.16801583]
[null,"UC-35","10",391,1111,28.882,228.96465438,61.23528,1502,1530.882,1759.84665438,1821.0819343800001]
[null,"DHC-7 ","10",1213,4271,86.646,228.96465438,222.82584,5484,5570.646,5799.61065438,6022.43649438]
[]
[null,"FY10 DOD Rotary Wing Aviation Reimbursable Rates"]
[null,"Aircraft","FY","Fuel","DLR","Other Consumables","Depot Maintenance","Other CLS per MH","Crew Pay","Asset Utilization","DoD Rate","Other FED AGY","FMS","Public Rate"]
[null,"AH-64A                        ","10",326.453645320197,4109.52,1125.99,2192.7980431808987,923.7348327998288,171.60469293,354.00404856923694,8678.496521300924,8850.101214230923,8850.101214230923,9204.10526280016]
[null,"AH-64D                        ","10",352.3781258399511,2283.19,719.0899999999999,2192.7980431808987,923.7348327998288,171.60469293,265.71182779002714,6471.191001820679,6642.795694750679,6642.795694750679,6908.507522540706]
[null,"CH-47D                        ","10",964.9613793103449,3955.51,1559.42,2623.8981939928053,1187.9557307052746,286.32461582999997,423.1227967935371,10291.745304008426,10578.069919838426,10578.069919838426,11001.192716631964]
[null,"CH-47F                   ","10",964.9613793103449,4154.64,1760.9700000000003,2623.8981939928053,1187.9557307052746,143.16230791499999,433.423504476937,10692.425304008426,10835.587611923425,10835.587611923425,11269.011116400363]
[null,"OH-58C                        ","10",62.03881773399015,226.72,110.27,622.3619315325602,391.39337220143017,143.16230791499999,62.23785717531921,1412.7841214679804,1555.9464293829803,1555.9464293829803,1618.1842865582996]
[null,"OH-58D                        ","10",101.10300702307582,1027.6,291.83,622.3619315325602,391.39337220143017,228.96465438,106.53011860548264,2434.288310757066,2663.252965137066,2663.252965137066,2769.7830837425486]
[null,"TH-67","10",83.10704885878536,224.62910759766103,0,0,218.5229013639197,171.60469293,27.914550030014645,526.259057820366,697.8637507503661,697.8637507503661,725.7783007803807]
[null,"UH-1H                         ","10",224.6907881773399,518.74,307.42,1663.832574246824,744.9894041030027,228.96465438,147.54549683628667,3459.6727665271665,3688.6374209071664,3688.6374209071664,3836.182917743453]
[null,"UH-60A                        ","10",320.2188669950738,1944.87,544.51,1663.832574246824,800.8087292513168,228.96465438,220.12819299492858,5274.2401704932145,5503.204824873214,5503.204824873214,5723.333017868143]
[null,"UH-60L                        ","10",320.2188669950738,1341.13,416.65,1663.832574246824,800.8087292513168,228.96465438,190.86419299492857,4542.640170493214,4771.604824873214,4771.604824873214,4962.469017868143]
[null,"UH-60M","10",320.2188669950738,1471.55,376.7,1663.832574246824,744.9894041030027,228.96465438,192.25021998899604,4577.290845344901,4806.255499724901,4806.255499724901,4998.505719713897]